**Product Description**

KY-008 Laser Transmitter Module:   
Operating voltage:5V  
Output wavelength:650 nm  
3 pins module  
Size: 15 \* 24mm  
Laser Receiver Sensor Module:   
Supply Voltage: 5V.Size: 15.2x22.2mm/0.60x0.84Inches.   
Output:Output high level when there is laser irradiation.Output low level when no laser irradiation.   
When the laser irradiation, the high level action relay module does not operate.Relay module action with high level action when laser front irradiates: relay module action with high level action when laser back irradiates.   
  
Package Includes:2Sets  
2Pc x KY-008 Laser Transmitter Module  
2Pc x Laser Receiver Sensor Module